**Glasswasher PROFI with integrated water softener**

**Model: Profi GXS-10B**

|  |  |
| --- | --- |
| Type | One Tank Glasswasher with integrated water softener |
| Rack Size | 500x500 mm  |
| Design | Front door machine, adjustable as undercounter model  |
| Capacity | 60 Racks/h / 2160 Glasses/h  |
| Voltage | 400/50/3 (230/50/1)  |
| Tank, Frame and Panels | Stainless steel 18/9  |
| Wash result | According to DIN10512 section 7  |

|  |
| --- |
| Ready to install: |
| - fill and drain hoses- power cord (400 V-connection)- detergent dispenser- rinse agent dispenser- rinse pump- drain pump- non-return valve  |
| Wash pump with smart start Automatic Tank FillMulti-Phasing |
| **Rack equipment** |
| 1 Universal Glass Rack with 4 sloped rows 303171, plastic coated steel wire |
| **Product Advantages** • **VISIOTRONIC-TOUCH control:**colour touchscreen (displays text and graphic) in conjunction with single-button control and remaining cycle time indication.• **WASHSMART APP:** controlling your warewash operation with smart technology: status and messages,usage and operating costs, hygiene, service and consumables order• **SENSO-ACTIVE resource management:** constantly measuresthe quality of the wash water andkeeps the amount of rinsing neededin each rinse cycle to the minimumin order to guarantee a fully hygienicwash result• **CLIP-IN wash and rinse arms**: wash and rinse arms can be removed with one hand and without any tools• **Intelligent data documentation:**automatic recording of important operational data and consumptions and indication on the display• **USB-interface:** comfortable download of operational data in form of a protocol via USB• **GENIUS-X² fine filter system:**advanced filter system with prewash function reduces detergent consumption up to 35%• **Cold rinsing**: the rinse can be switched from hot to cold water so that you get cooler glasses without any loss of time• **Intensive programme**: intensive rinse cycle to wash glasses with critical design with raised fresh-wateramount• **Interlocked strainer**: prevents operation without tank strainer• **Optional refill signal:** monitors contents of external as well as integrated chemical containers• **Hygiene programme:** for removal of calcium carbonate and other deposits from wash chamber |

|  |
| --- |
| **Technical Data:**  |
| Machine housing width | 600 mm |
| Machine housing Depth | 603 mm |
| Depth when Door is open | 1048 mm |
| Height | 825 mm |
| Loading height | 425 mm |
|   |
| Cycle time\*\* | 60 / 90 / 120 sec. and special programs |
| Capacity\*\* | Up to 60 Racks/h / 2160 Glasses/h |
| Wash temperature | 55 °C |
| Rinse temperature | 65 °C |
| Tank capacity | 11,6 l |
| Fresh water consumption/Rack | 2 l |
|   |
| Booster loading | 6,2 kW (2,1 kW) |
| Total loading | 6,8 kW (2,7 kW) |
| Pump power | 0,5 kW / 350 l/min |
| - | 3x16 A (16 A) |
| Voltage | 400/50/3 (230/50/1) |
|   |
| \* To reach set rinse temperatures even with cold water connection, the actual cycle-times extend accordingly.  |
| \*\* Theoretical performance  |

